#
SUNROOF MOTOR REMOVAL/INSTALLATION

BHE091569873W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (3) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (4) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (6) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (7) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (8) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (9) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (10) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (11) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

3. Disconnect the sunroof motor connector.

4. Remove the screws, then remove the sunroof motor.

5. Install in the reverse order of removal.

  Note

  • If the glass panel or the sunroof motor is moved with the sunroof motor removed, initial position setting of the sunroof motor will be required. Perform initial position setting referring to the Sunroof Motor Assembly Note. (See Sunroof Motor Assembly Note.)