#
DTC C1093

BHE040243000W18

DTC | C1093 | DSC OFF switch
DETECTION CONDITION | • Continuous ON signal from the DSC OFF switch for 5 s or more is detected.
POSSIBLE CAUSE | • The driver pressed and held the DSC OFF switch for 5 s or more. • Short to ground in the wiring harness between the DSC HU/CM terminal AP and the DSC OFF switch terminal C • DSC OFF switch malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT DSC HU/CM TO DSC OFF SWITCH FOR SHORT TO GROUND • Turn the ignition switch off. • Disconnect DSC HU/CM and DSC OFF switch connector. • Inspect for continuity between the DSC HU/CM terminal AP and ground. • Is there continuity? | Yes | Repair or replace the wiring harness for short to ground between DSC HU/CM terminal AP and DSC OFF switch terminal C, then go to the next step.
No | Go to the next step.
2 | INSPECT DSC OFF SWITCH • Inspect the DSC OFF switch. (See DSC OFF SWITCH INSPECTION.) • Is the DSC OFF switch normal? | Yes | Go to the next step.
No | Replace the DSC OFF switch, then go to the next step. (See DSC OFF SWITCH REMOVAL/INSTALLATION.)
3 | VERIFY TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the memory. (See Clearing DTCs Procedures.) • Is the same DTC present? | Yes | Replace the DSC HU/CM, then go to the next step. (See DSC HU/CM REMOVAL/INSTALLATION.)
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Are any other DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.