#
FRONT FOG LIGHT SWITCH INSPECTION

BHE091866402W01

## Light Switch (LH)

1. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Remove the ignition key illumination. (See IGNITION KEY ILLUMINATION BULB REMOVAL/INSTALLATION.)

3. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the light switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the light switch.

## Light Switch (RH)

1. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Remove the ignition key illumination. (See IGNITION KEY ILLUMINATION BULB REMOVAL/INSTALLATION.)

3. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

4. Verify that the continuity between the light switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the light switch.