#
ENGINE TECHNICAL DATA

BHE015001001E01

ITEMS | ENGINE TYPE
--- | ---
13B-MSP
STANDARD POWER | HIGH POWER
SIDE HOUSING (FRONT, INTERMEDIATE, REAR) INSPECTION
Maximum distortion | (mm {in}) | 0.04 {0.0016}
Maximum wear (Vertical wear) | (mm {in}) | 0.10 {0.0039}
Maximum wear (Convex oval) | (mm {in}) | Oil seal inner path | 0.01 {0.0004}
Oil seal outer path | 0.10 {0.0039}
Maximum wear (Oil seal stepped path wear) | (mm {in}) | 0.02 {0.0008}
ROTOR HOUSING
Maximum width difference | (mm {in}) | 0.06 {0.0024}
ROTOR
Rotor and side housing clearance | (mm {in}) | Standard | 0.05-0.19 {0.0020-0.0074}
Maximum | 0.05 {0.002}
Protrusion of the rotor round | (mm {in}) | Standard | 0.12-0.18 {0.0048-0.0070}
Minimum | 0.1 {0.0039}
Apex seal groove and the apex seal clearance | (mm {in}) | Standard | 0.042-0.101 {0.0017-0.0039}
Maximum | 0.15 {0.0059}
APEX SEAL, APEX SEAL SPRING
Apex seal height | (mm {in}) | Standard | 5.3 {0.20}
Minimum | 4.3 {0.17}
Apex seal spring height | (mm {in}) | Standard | 5.4 {0.213}
Minimum | 3.5 {0.148}
CORNER SEAL, CORNER SEAL SPRING
Minimum projection of the corner seal | (mm {in}) | 0.5 {0.02}
SIDE SEAL, SIDE SEAL SPRING
Corner seal and side seal clearance | (mm {in}) | Standard | 0.05-0.15 {0.0020-0.0059}
Maximum | 0.4 {0.016}
Minimum projection of the side seal | (mm {in}) | 0.5 {0.02}
CUT-OFF SEAL, CUT OFF SEAL SPRING
Cut-off seal height | (mm {in}) | Standard | 3.95 {0.1555}
Minimum | 3.8 {0.15}
Minimum projection of the cut off seal | (mm {in}) | 0.5 {0.02}
OIL SEAL, OIL SEAL SPRING
Maximum contact width | (mm {in}) | 0.5 {0.02}
Maximum circumferential width | (mm {in}) | 2.5 {0.098} (or 10 nicks or more)
Minimum projection of the oil seal | (mm {in}) | 0.5 {0.02}
ECCENTRIC SHAFT
Main bearing oil clearance | (mm {in}) | Standard | 0.055-0.075 {0.0022-0.0029} | 0.045-0.085 {0.0018-0.0033}
Maximum | 0.1 {0.0039 in}
Rotor bearing oil clearance | (mm {in}) | Standard | 0.06-0.08 {0.0024-0.0030}
Maximum | 0.1 {0.0039}
Runout | (mm {in}) | Standard | 0.02 {0.0008}
Maximum | 0.06 {0.0024}
End play | (mm {in}) | Standard | 0.04-0.09 {0.0016-0.0035}
Maximum | 0.1 {0.0039}
ECCENTRIC SHAFT BYPASS VALVE
Minimum projection | (mm {in}) | 6 {0.24}
OIL PUMP
Side clearance | (mm {in}) | Standard | 0.20-0.25 {0.0079-0.0098}
Maximum | 0.3 {0.0118}
Tip clearance | (mm {in}) | Standard | 0.03-0.12 {0.0012-0.0047}
Maximum | 0.15 {0.0059}
Body clearance | (mm {in}) | Standard | 0.03-0.125 {0.0012-0.0049}
Maximum | 0.15 {0.0059}