#
AUDIO CONTROL SWITCH INSPECTION

BHE092000148W02

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the audio control switch connector.

4. Verify the resistance and continuity between the audio control switch terminals.

  • If the resistance and continuity are not as indicated in the tables, replace the audio control light switch.

  R :
Resistance. See the table.

Switch position | Resistance (ohm)
--- | ---
VOL- switch ON | 51-56
VOL+ switch ON | 140-154
SEEK+ switch ON | 286-315
SEEK- switch ON | 534-589
MODE switch ON | 985-1,080
MUTE switch ON | 1,940-2,130
OFF | 4,800-5,290