#
HVAC CONTROL SYSTEM [MANUAL AIR CONDITIONER]

BHE074001042W02

1 | Air intake actuator (See AIR INTAKE ACTUATOR REMOVAL/INSTALLATION.) (See AIR INTAKE ACTUATOR INSPECTION.)
2 | Air mix actuator (See AIR MIX ACTUATOR REMOVAL/INSTALLATION.) (See AIR MIX ACTUATOR INSPECTION.)
3 | Airflow mode actuator (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION.) (See AIRFLOW MODE ACTUATOR INSPECTION.)
4 | Blower motor (See BLOWER MOTOR REMOVAL/INSTALLATION.) (See BLOWER MOTOR INSPECTION.)
5 | Resistor (See RESISTOR REMOVAL/INSTALLATION.) (See RESISTOR INSPECTION.)
6 | Magnetic clutch (See MAGNETIC CLUTCH ADJUSTMENT.) (See MAGNETIC CLUTCH INSPECTION.)
7 | Ambient temperature sensor (See AMBIENT TEMPERATURE SENSOR REMOVAL/INSTALLATION.) (See AMBIENT TEMPERATURE SENSOR INSPECTION.)
8 | Evaporator temperature sensor (See EVAPORATOR TEMPERATURE SENSOR REMOVAL/INSTALLATION.) (See EVAPORATOR TEMPERATURE SENSOR INSPECTION.)
9 | Refrigerant pressure switch (See REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION.) (See REFRIGERANT PRESSURE SWITCH INSPECTION.)
10 | Climate control unit (See CLIMATE CONTROL UNIT REMOVAL/INSTALLATION.) (See CLIMATE CONTROL UNIT INSPECTION.)
11 | A/C amplifier (See A/C AMPLIFIER INSPECTION [MANUAL AIR CONDITIONER].)
12 | A/C relay (See RELAY INSPECTION.)
13 | Blower relay (See RELAY INSPECTION.)