#
HEADLIGHT CLEANER ACTUATOR REMOVAL/INSTALLATION

BHE091966122W07

1. Disconnect the negative battery cable.

2. Remove the front side turn light. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove the headlight cleaner nozzle. (See HEADLIGHT CLEANER NOZZLE REMOVAL.) (SeeHEADLIGHT CLEANER NOZZLE INSTALLATION.)

5. Squeeze the clip tabs and slide the clip in the direction of the arrow.

6. Disconnect headlight cleaner hose from the headlight cleaner actuator.

7. Remove the screw, then remove the headlight cleaner actuator.

8. Install in the reverse order of removal.