#
MANUAL TRANSMISSION SPECIFICATION [R15M-D]

BHE050001030T04

Item | Specifications
--- | ---
Transmission type | R15M-D
Transmission control | Floor-shift
Shift assist | Synchromesh
Gear ratio | 1GR | 3.483
2GR | 2.015
3GR | 1.391
4GR | 1.000
5GR | 0.806
Reverse | 3.288
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10°C {50°F} | SAE 80W-90
Capacity (approx. quantity) | (L {US qt, lmp qt}) | 2.5 {2.6, 2.2}