#
GENERAL PROCEDURES (CLUTCH)

BHE051016003W02

  Caution

  • Fluid will damage painted surfaces. Be careful not to spill any on painted surfaces. If fluid does get on painted surfaces, wipe it off immediately.

  Note

  • If any hydraulic related parts of the clutch system are removed during the procedure, add brake fluid, bleed the system and inspect for leakage after the procedure has been completed.

1. Remove the clutch pipe using the SST (49 0259 770B).

2. Install the clutch pipe using a torque wrench and the SST (49 0259 770B).