#
REAR SPEAKER REMOVAL/INSTALLATION

BHE092066961W03

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Remove the tire house trim. (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Remove the rear pillar trim. (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (5) Remove the rear package center trim, the rear package side trim. (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Rear door speaker

4. Install in the reverse order of removal.