#
ON-BOARD DIAGNOSTIC SYSTEM PID/DATA MONITOR FUNCTION (DYNAMIC STABILITY CONTROL)

BHE040243000T03

• The PID/data monitor function is used for optionally selecting input/output signal monitor items preset in the DSC HU/CM and reading them out in real-time.

## PID/DATA Monitor Table

PID/data monitor item | Input/output part | Unit/Condition (Tester display)
--- | --- | ---
ABS_LAMP | ABS warning light | On/Off
ABS_VOLT | Battery | V
ABSLF_I | LF inlet solenoid valve | On/Off
ABSLF_O | LF outlet solenoid valve | On/Off
ABSLR_I | LR inlet solenoid valve | On/Off
ABSLR_O | LR outlet solenoid valve | On/Off
ABSRF_I | RF inlet solenoid valve | On/Off
ABSRF_O | RF outlet solenoid valve | On/Off
ABSRR_I | RR inlet solenoid valve | On/Off
ABSRR_O | RR outlet solenoid valve | On/Off
BOO_ABS | Brake switch | On/Off
BRAKE_LMP | Brake system warning light | On/Off
CCNTABS | Number of continuous DTCs | -
L_DSC O | LH stability control solenoid valve | On/Off
LAT ACC | Combined sensor (Lateral-G) | G
LF_WSPD | ABS wheel-speed sensor (LF) | KPH, MPH
LR_WSPD | ABS wheel-speed sensor (LR) | KPH, MPH
MCYLIP | Brake fluid pressure sensor | kPa, psi, Bar
PMPSTAT | Pump motor | On/Off
R_DSC O | RH stability control solenoid valve | On/Off
RF_WSPD | ABS wheel-speed sensor (RF) | KPH, MPH
RPM | PCM (engine speed) | RPM
RR_WSPD | ABS wheel-speed sensor (RR) | KPH, MPH
SWA POS | Steering angle sensor | °
TC LVAL | LH traction switch solenoid valve | On/Off
TC RVAL | RH traction switch solenoid valve | On/Off
TPI | PCM (throttle opening angle) | %
YAW_RATE | Combined sensor (yaw rate) | deg./s