#
ENGINE OIL LEVEL INSPECTION

BHE011114001W01

1. Position the vehicle on level ground.

2. Warm up the engine.

3. Stop the engine and allow approx. 5 min before continuing.

4. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

5. Remove the dipstick and verify that the oil level is between the F and L marks on the dipstick.

  • If the oil level is below the L mark, add oil.

6. Install the dipstick.

7. Install the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)