#
MASTER CYLINDER CONSTRUCTION

BHE041143400T01

• A plunger-type master cylinder with a 22.22 mm {0.875 in} bore has been adopted, improving durability.

  Note

  • Plunger type: A system where the cups are fixed on the cylinder, and the piston slides through the inner perimeter of the cups.

• The master cylinder outlet pipe diameter has been increased, improving response during DSC operation.

• Except for the reservoir, the master cylinder cannot be disassembled. Therefore, if there is any malfunction in the interior of the master cylinder, replace the cylinder component without disassembling.

1 | Reserve tank
2 | Cylinder component