#
AUXILIARY PORT VALVE (APV) MOTOR CONSTRUCTION/OPERATION (13B-MSP (HIGH POWER))

BHE011320130T08

• The position sensor is built into the APV motor.

• The motor is driven according to an operation signal from the PCM.

• The motor driving force is transmitted to the drive gear, counter gear, shaft, and arm, thereby opening or closing the APV.

1 | APV motor
2 | Counter gear
3 | Close
4 | Open
5 | APV
6 | Arm
7 | Shaft
8 | Drive gear