#
FUEL-FILLER LID OPENER REMOVAL/INSTALLATION

BHE091466640W01

1. To remove the fuel-filler lid opener, remove the trunk side trim (LH). (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

2. When removing the fuel-filler lid opener lever, perform the following procedure:

  (1) Remove the inner scuff plate (driver's side). (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Remove the front side trim (driver's side). (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)
  (3) Remove the fasteners and the wiring harness clips, and then partially peel back the floor covering so that the fuel-filler lid opener lever can be removed.

3. When removing the fuel-filler lid opener cable, perform the following procedure:

  (1) Partially peel back the trunk mat.
  (2) Remove the rear seat (driver's side). (SeeREAR SEAT REMOVAL/INSTALLATION)
  (3) Remove the tire house trim (driver's side). (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Partially peel back the floor covering so that the fuel-filler lid opener cable can be removed.

4. Remove in the order indicated in the table.

1 | Stopper bracket
2 | Fuel-filler lid opener
3 | Fuel-filler lid opener lever
4 | Fuel-filler lid opener cable

5. Install in the reverse order of removal.

6. Adjust the fuel-filler lid. (See FUEL-FILLER LID ADJUSTMENT.)