#
LUBRICATION SYSTEM OUTLINE

BHE051319900T01

• In the conventional system, the rear section is lubricated by ATF returning from the ATF oil cooler. In the new system, all parts are lubricated directly from the control valve.

• With this construction, the system is unaffected by the ATF oil cooler, and thus a steady amount of lubricant is supplied.

1 | Front lubrication
2 | Rear lubrication
3 | Extension housing lubrication
4 | Control valve body
5 | Oil cooler

• A passage located in the rear of the extension housing supplies a steady amount of lubricant exclusively to the bushing.

1 | Bushing lubrication passage