#
PCM CONSTRUCTION/OPERATION

BHE014018880T02

• Located in front area of the engine compartment.

• 122-pin connector (13B-MSP (High Power)) or 105-pin connector (13B-MSP (Standard Power)) is used for the PCM.

1 | (13B-MSP (High power))

• The fresh air induction duct has been installed to cool the PCM. During regular driving, fresh air is induced by wind that blows against the vehicle as it is running. When the PCM temperature is high and the vehicle has stopped, the cooling fan operates, inducing additional fresh air.

1 | PCM
2 | Duct
3 | Battery