#
ECCENTRIC SHAFT END PLAY INSPECTION

BHE011011D01E02

1. Lock the flywheel (MT) or counterweight (AT) against rotation using the SST.

2. Assemble the parts in the following order:

  (1) Spacer
  (2) Needle bearing
  (3) Thrust plate
  (4) Balance weight
  (5) Oil pump drive gear
  (6) Metering oil pump drive gear

  Caution

  • When assembling the spacer, do not allow the spacer to be caught in the needle bearing in the plate.

3. Assemble the eccentric shaft pulley, eccentric shaft position plate, pulley boss component apply engine oil to the pulley lockbolt threads, and then tighten.

  Tightening torque
  300-340 N·m {30.6-34.6 kgf·m, 222-250 ft·lbf}

4. Remove the SST.

5. Measure the end play of the eccentric shaft using a dial gauge.

  • If not within the specification, replace the spacer with one that is thicker than the currently assembled one. If it exceeds the specification, replace with a thinner spacer.

  Standard end play
  0.04-0.09 mm {0.0016-0.0035 in}
  Maximum end play
  0.1 mm {0.0039 in}

Spacer types

(mm {in})

Marking | Dimension
--- | ---
A | 7.985 {0.3144}
B | 8.005 {0.3152}
C | 8.025 {0.3159}
D | 8.045 {0.3167}
E | 8.065 {0.3175}

  Note

  • If the end play is not within the specification even after replacing with an A-marked spacer, adjust by grinding it and reuse.