#
FRONT SEAT REMOVAL/INSTALLATION

BHE091357100W01

  Warning

  • Handling the front seat (with a side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read the service warnings before handling the front seat (with a side air bag). (See SERVICE WARNINGS.)

1. Turn the ignition switch to the LOCK position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Disconnect the connector.

4. Remove the covers.

5. Remove the bolts, then remove the front seat.

6. Install in the reverse order of removal.