#
FRONT BUMPER DISASSEMBLY/ASSEMBLY

BHE091050010W02

1. To disassemble the front bumper, remove the following parts:

  (1) Front fog lights (Vehicles with the front fog lights)(See FRONT FOG LIGHT REMOVAL/INSTALLATION.)
  (2) Headlight cleaner hose (Vehicles with the headlight cleaner)(See HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION.)
  (3) Headlight cleaner nozzles (Vehicles with the headlight cleaner)(See HEADLIGHT CLEANER NOZZLE REMOVAL.)(SeeHEADLIGHT CLEANER NOZZLE INSTALLATION.)
  (4) Headlight cleaner actuator (Vehicles with the headlight cleaner)(See HEADLIGHT CLEANER ACTUATOR REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

1 | Screw A
2 | Airdam skirt
3 | Bolt A
4 | License plate holder
5 | Fastener
6 | Front bumper mesh
7 | Bolt B
8 | Set plate
9 | Front bumper retainer No.1
10 | Screw B
11 | Screw C
12 | Front fog light hole cover
13 | Front bumper fascia

3. Assemble in the reverse order of disassembly.