#
TRANSMISSION/TRANSAXLE TECHNICAL DATA

BHE055001024W01

Item | Specifications
--- | ---
CLUTCH
Clutch pedal | Free play | Pedal free play | (mm {in}) | 5-15 {0.20-0.59}
Push rod free play | At push rod setting line | (mm {in}) | 0.1-0.5 {0.004-0.02} (Reference value)
At clutch pedal pad | (mm {in}) | 0.5-2.9 {0.02-0.11}
Disengagement point | Disengagement stroke | (mm {in}) | 111.8 {4.402} (Reference value)
Pedal stroke | (mm {in}) | 130 {5.12} (Reference value)
Clutch cover | Diaphragm spring fingers | Depth | (mm {in}) | 0.6 {0.024}
Maximum height difference | (mm {in}) | 1.0 {0.039}
Maximum clearance of flatness of the pressure plate | (mm {in}) | 0.5 {0.020}
Clutch disc | Minimum thickness | (mm {in}) | 0.3 {0.012}
Run out limit | (mm {in}) | 0.7 {0.028}
Flywheel | Run out limit | (mm {in}) | 0.2 {0.008}
Clutch fluid | Type |  | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian specs.: SAE J1703, FMVSS 116 DOT-3
MANUAL TRANSMISSION
Manual transmission type | R15M-D
Oil | Grade | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (Approximate quantity) | Transmission case | (L {US qt, lmp qt}) | 2.5 {2.6, 2.2}
Control case | (ml {cu in}) | 290-320 {17.7-19.5}
Manual transmission type | Y16M-D
Oil | Grade | API Service GL-4 or GL-5
Viscosity | All-season | SAE 75W-90
Capacity (Approximate quantity) | 1.75 {1.85, 1.54}}
(L {US qt, lmp qt})
AUTOMATIC TRANSMISSION
Automatic transmission type | RC4A-EL
ATF | Type | ATF M-III or equivalent (e.g. DexronII)
Capacity (Approx. quantity) | 8.7 {9.2, 7.7}
(L {US qt, lmp qt})
Line pressure | D, M range | Idle | 320-450 {3.3-4.6, 46-65}
Stall | 1,130-1,330 {11.5-13.6, 164-193}
(kPa {kgf/cm2, psi}) | R position | Idle | 380-580 {3.9-5.9, 55-84}
Stall | 1,470-1,700 {15.0-17.3, 213-247}
P, N position | Idle | 380-580 {3.9-5.9, 55-84}
Engine stall speed | (rpm) | D, M range | 2,400-2,900
R position
Time lag | (s) | N position→ D range | approx. 0.2-1.3
N position→ R position | approx. 0.2-1.3
Transmission Fluid temperature (TFT) sensor (kilohm) | ATF temperature: -20 °C {-4 °F} | 15.87-17.54
ATF temperature: 0 °C {32 °F} | 5.727-6.329
ATF temperature: 20 °C {68 °F} | 2.375-2.625
ATF temperature: 40 °C {104 °F} | 1.102-1.218
ATF temperature: 60 °C {140 °F} | 0.561-0.620
ATF temperature: 80 °C {176 °F} | 0.308-0.341
ATF temperature: 100 °C {212 °F} | 0.181-0.200
ATF temperature: 120 °C {248 °F} | 0.112-0.123
ATF temperature: 130 °C {266 °F} | 0.089-0.099
Turbine sensor (ohm) | M range, 1st gear at 20 km/h {12 mph} | 7
Vehicle speedometer sensor (VSS) (ohm) | M range, 1st gear at 20 km/h {12 mph} | 7
Solenoid valves ATF temperature: 20-80 °C {68-176 °F} | (ohm) | Shift solenoid A | 2.7-4.4
Shift solenoid B | 2.7-4.4
Shift solenoid C | 2.7-4.4
Shift solenoid F | 2.7-4.4
Pressure control solenoid | 12.3-16.3
TCC control solenoid | 12.1-16.0