#
FRONT SEAT DISASSEMBLY/ASSEMBLY

BHE091357100W02

  Warning

  • Handling the front seat (with a side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read the service warnings before handling the front seat (with a side air bag). (See SERVICE WARNINGS.)

1. For vehicles with side air bags, remove the side air bag module. (See SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

2. Disassemble in the order indicated in the table.

3. Assemble in the reverse order of disassembly.

## Manual Seat (Driver's Seat)

1 | Recliner dial (dial type) /Recliner lever (lever type)
2 | Outer lift lever
3 | Inner lift lever
4 | Side cover
5 | Reverse cover
6 | Front buckle
7 | Cover
8 | Seat back trim
9 | Seat back pad
10 | Seat back frame
11 | Side air bag cover
12 | Seat cushion trim
13 | Seat cushion pad
14 | Seat cushion frame
15 | Slide adjuster

## Power Seat (Driver's Seat)

1 | Slider switch knob
2 | Recliner switch knob
3 | Lumbar support switch knob
4 | Side cover
5 | Reverse cover
6 | Front cover
7 | Power seat switch
8 | Front buckle
9 | Cover
10 | Seat back cover
11 | Seat back trim
12 | Seat warmer unit
13 | Seat back pad
14 | Seat back frame
15 | Side air bag cover
16 | Lumbar support motor
17 | Seat back hardboard
18 | Seat cushion trim
19 | Seat warmer unit
20 | Seat cushion pad
21 | Seat cushion frame
22 | Slide adjuster

## Manual Seat (Passenger's Seat)

1 | Recliner lever
2 | Side cover
3 | Reverse cover
4 | Front buckle
5 | Cover
6 | Seat back trim
7 | Seat back pad
8 | Seat back frame
9 | Side air bag cover
10 | Seat cushion trim
11 | Seat cushion pad
12 | Seat cushion frame
13 | Slide adjuster