#
UNDERBODY FLAT-PLANE DIMENSIONS

BHE098053010B01

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame standard hole | ø9.8 {0.39}
B | Crossmember No.1 standard hole | ø7 {0.28}
C | Front crossmember mounting bolt | M14 {0.55}
D | Front suspension mounting block | ø44 {1.73}
E | Front crossmember mounting bolt | M14 {0.55}
F | Front frame rear standard hole | ø16 {0.63}
G | Front frame rear standard hole | 16 × 20
{0.63 × 0.79}
H | Front B frame standard hole | M14 {0.55}
I | Front B frame standard hole | ø20 {0.79}
J | Rear side frame standard hole | ø16 {0.63}
K | Rear crossmember mounting bolt | M14 {0.55}
L | Rear crossmember mounting bolt | M14 {0.55}
M | Rear suspension mounting block | ø97 {3.82}
N | Rear crossmember mounting bolt | M14 {0.55}
O | Bumper bracket standard hole | 14 × 10
{0.55 × 0.39}