#
DTC B1342

BHE080201046W09

DTC B1342 | • SAS unit (air bag system warning light DTC 12 is displayed.) • SAS unit DTC 12 detection circuit malfunction (the air bag system warning light illuminates continuously.)
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • Malfunction in the SAS unit internal circuit
POSSIBLE CAUSE | • SAS unit malfunction

Diagnostic procedure

ACTION
• Replace the SAS unit. (See SAS UNIT REMOVAL/INSTALLATION)