#
DRIVE MODE DETERMINATION OPERATION

BHE051318901T06

D range

• When the ATF temperature is high or low, the mode is automatically switched to each shift pattern: when the ATF temperature is high, the TCC point is shifted to the low speed side, and when the ATF temperature is low, 4GR is inhibited.

M range

• When the selector lever is shifted over from the D to M range position, the M range switch in the selector lever component turns on, sending a manual mode command signal to the TCM which activates the manual mode shift control.