#
DISC PAD (REAR) REPLACEMENT

BHE041126630W01

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, depress the brake pedal a few times, and inspect the following.

  – The disc pad projection is securely installed to the piston groove
  – Parking brake lever stroke
  – Brake drag

1 | Parking brake cable (See Parking Brake Cable Installation Note.)
2 | Bolt
3 | Caliper (See Caliper Installation Note.)
4 | Disc pad
5 | Shim
6 | Guide plate

## Caliper Installation Note

1. Clean the exposed area of the piston.

2. Rotate the piston clockwise slowly using the SST and push in the piston completely until the piston grooves are in the position shown in the figure.

3. Install the caliper.