#
FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

BHE091050070W01

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove fasteners A, then remove the energy-absorbing foam.

5. Remove fasteners B, then remove front bumper retainer No.2.

6. Remove the bolts, then remove the front bumper reinforcement.

7. Install in the reverse order of removal.