#
PUNCTURE REPAIR KIT OUTLINE

BHE021237100T01

• An emergency puncture repair kit has been provided for all models instead of a temporary spare tire. This kit enables temporary repair of a puncture without tire removal.

• The emergency puncture repair kit is located in the trunk compartment and includes the following:

1 | Emergency puncture repair kit

  – Repair agent
  – Repair agent filler hose
  – Air compressor
  – Tire valve core
  – Tire valve core tool
  – Instruction manual
  – Speed limit label
  – Filled tire indication label

• The accessory socket (12V DC) is used as an input power source for the air compressor and the compressor plug includes a 10 A fuse.

  Note

  • The expiration date of the repair agent is printed on the repair agent bottle. Do not use the repair agent if it has passed the expiration date.
  • Dispose of repair agent according to local waste disposal law.
  • The repair agent consists of the following ingredients:

  – Deproteinized natural rubber latex
  – Emulsified adhesive resin
  – Propylene glycol