#
REAR SEAT BELT REMOVAL/INSTALLATION

BHE081157630W04

  Caution

  • The ELR (emergency locking retractor) has a spring that will unwind if the retractor cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

1. Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION.)

2. Remove the front console. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove the rear console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the rear package trim. (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Bolt
2 | Rear seat belt

6. Install in the reverse order of removal.