#
KEYLESS UNIT REMOVAL/INSTALLATION

BHE091467820W01

## L.H.D.

1. When replacing the keyless unit, perform the following procedure:

  • KEYLESS UNIT CONFIGURATION

2. Disconnect the negative battery cable.

3. Remove the front side trim. (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the nut and clip.

5. Remove the connector clip installed to the bracket by shifting the keyless unit downward.

6. Disconnect the keyless unit connector.

7. Push the stopper with a small screwdriver and remove the bracket in the direction shown by the arrow.

8. Install in the reverse order of removal.

9. When replacing the keyless unit, perform the following procedure:

  • IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.
  • TRANSMITTER ID CODE CHANGE.

## R.H.D.

1. When replacing the keyless unit, perform the following procedure:

  • KEYLESS UNIT CONFIGURATION

2. Disconnect the negative battery cable.

3. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

4. Remove the bolts.

5. Remove the connector clip installed to the bracket by shifting the keyless unit downward.

6. Disconnect the keyless unit connector.

7. Push the stopper with a small screwdriver and remove the bracket in the direction shown by the arrow.

8. Install in the reverse order of removal.

9. When replacing the keyless unit, perform the following procedure:

  • IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.
  • TRANSMITTER ID CODE CHANGE.