#
SIDE PANEL REMOVAL/INSTALLATION

BHE091765271W01

1. Remove the inner scuff plate. (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)

2. Remove the front side trim. (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

3. Detach clips A and B, using a flathead screwdriver wrapped with protective tape.

4. Pull the side panel outward and detach tab C from the dashboard, then remove the side panel.

5. Install in the reverse order of removal.