#
TRANSMISSION RANGE (TR) SWITCH INSPECTION

BHE051319200W01

## Operating inspection

1. Verify that the starter operates only when the ignition switch is turned to the START position with the selector lever in the P or N position.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT.)

2. Verify that the back-up lights illuminate when shifted to the R position with the ignition switch at the ON position.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT.)

3. Verify that the positions of the selector lever and the indicator are aligned.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT.)

## Continuity Inspection

  Caution

  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable.

4. Remove the catalytic converter.

(See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

5. Remove the insulator.

6. Disconnect the TR switch connector.

7. Verify continuity as indicated in the table.

  • If there is any malfunction, adjust the TR switch. (See TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT.)

8. Reinspect for continuity at TR switch.

  • If there is any malfunction, replace the TR switch. (See TRANSMISSION RANGE (TR) SWITCH REMOVAL/INSTALLATION.)

9. Connect the TR switch connector.

10. Install the insulator.

  Tightening torque
  8-11 N·m {82-112 kgf·cm, 72-97 in·lbf}

11. Install the catalytic converter.

(See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

12. Connect the negative battery cable.

13. Install the battery cover.

14. Install the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)