#
TENSION BOLT CONSTRUCTION

BHE011010908T05

• The tension bolts, pointed from the rear to the front housing, are tightened to fix the housings.

• Corrugation at the center of the tension bolts prevents resonance.

• There are two types of tension bolt lengths, with the longer bolts having a hole in the bolt head for differentiating between the two types of lengths.

1 | Corrugation
2 | Tension bolt
3 | Seal washer
4 | Other bolt type
5 | No.18 bolt
6 | Identification hole