#
DTC TABLE [RC4A-EL]

BHE050201026W05
×: Available

DTC No. | Condition | MIL | AT warning light illuminated | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0705 | Transmission range (TR) switch circuit malfunction (short to power supply) | ON | YES | 2 | CCM | × | (See DTC P0705.)
P0706 | Transmission range (TR) switch circuit malfunction (open circuit/short to ground) | ON | YES | 2 | CCM | × | (See DTC P0706.)
P0707 | M range switch, up switch or down switch circuit malfunction (open circuit/short to ground) | OFF | YES | 1 | CCM | × | (See DTC P0707.)
P0708 | Steering shift switch circuit malfunction (open circuit/short to ground) | OFF | YES | 1 | CCM | × | (See DTC P0708.)
P0712 | Transmission fluid temperature (TFT) sensor circuit malfunction (short to ground) | ON | YES | 1 | CCM | × | (See DTC P0712.)
P0713 | Transmission fluid temperature (TFT) sensor circuit malfunction (open circuit/short to power supply) | ON | YES | 1 | CCM | × | (See DTC P0713.)
P0715 | Turbine sensor circuit malfunction | ON | YES | 1 | CCM | × | (See DTC P0715.)
P0720 | Vehicle speed sensor (VSS) malfunction (open circuit/short to ground) | ON | YES | 1 | CCM | × | (See DTC P0720.)
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | OFF | NO | 1 | CCM | × | (See DTC P0731.)
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | OFF | NO | 1 | CCM | × | (See DTC P0732.)
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | OFF | NO | 1 | CCM | × | (See DTC P0733.)
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | OFF | NO | 1 | CCM | × | (See DTC P0734.)
P0743 | Torque converter clutch (TCC) solenoid valve circuit malfunction (open circuit/short to ground or power supply) | ON | YES | 1 | CCM | × | (See DTC P0743.)
P0748 | Pressure control solenoid circuit malfunction (open circuit/short to ground or power supply) | OFF | YES | 1 | CCM | × | (See DTC P0748.)
P0753 | Shift solenoid A circuit malfunction (open circuit/short to ground or power supply) | ON | YES | 1 | CCM | × | (See DTC P0753.)
P0758 | Shift solenoid F circuit malfunction (open circuit/short to ground or power supply) | ON | YES | 1 | CCM | × | (See DTC P0758.)
P0763 | Shift solenoid B circuit malfunction (open circuit/short to ground or power supply) | ON | YES | 1 | CCM | × | (See DTC P0763.)
P0768 | Shift solenoid C circuit malfunction (open circuit/short to ground or power supply) | ON | YES | 1 | CCM | × | (See DTC P0768.)
P0841 | Oil pressure switch B circuit malfunction | OFF | YES | 2 | CCM | × | (See DTC P0841.)
P0846 | Oil pressure switch C circuit malfunction | OFF | YES | 2 | CCM | × | (See DTC P0846.)
P0871 | Oil pressure switch F circuit malfunction | OFF | YES | 2 | CCM | × | (See DTC P0871.)
P0960 | GND return circuit malfunction | ON | YES | 1 | CCM | × | (See DTC P0960.)
P1759 | 2-4 brake fail-safe valve malfunction | OFF | YES | 2 | CCM | × | (See DTC P1759.)
P1764 | Low and reverse brake fail-safe valve malfunction | OFF | YES | 2 | CCM | × | (See DTC P1764.)
U0073 | CAN bus off | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)
U0100 | TCM cannot receive any signals from PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM].)

  MIL :
Malfunction Indicator Lamp
  DC :
Drive Cycle
  CCM :
Comprehensive Component Monitor