#
ENGINE DISASSEMBLY/ASSEMBLY

BHE011002000W05

1. Remove the engine from the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [R15M-D].) (See TRANSMISSION REMOVAL/INSTALLATION [Y16M-D].) (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION.)

2. Remove the following parts:

  (1) The clutch unit (MT) (See CLUTCH UNIT REMOVAL/INSTALLATION.)
  (2) The drive plate (AT) (See DRIVE PLATE REMOVAL/INSTALLATION.)
  (3) The intake-air system (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)
  (4) The exhaust system (See EXHAUST SYSTEM REMOVAL/INSTALLATION.)
  (5) The primary fuel injector and wiring harness (See FUEL INJECTOR REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Eccentric shaft position sensor (See ECCENTRIC SHAFT POSITION SENSOR REMOVAL/INSTALLATION.)
2 | A/C drive belt tensioner
3 | Oil hose
4 | Water pump pulley
5 | Generator strap
6 | Oil nozzle
7 | Metering oil pump (See METERING OIL PUMP REMOVAL/INSTALLATION.)
8 | Spark plug (See SPARK PLUG REMOVAL/INSTALLATION.)
9 | Knock sensor (See KNOCK SENSOR (KS) REMOVAL/INSTALLATION.)
10 | Oil pressure switch (See OIL PRESSURE INSPECTION.)
11 | Oil filler pipe