#
OBD PENDING TROUBLE CODE

BHE010200102W03

• These appear when a problem is detected in a monitored system. The code for a failed system is stored in the PCM memory in the first drive cycle. This code is called the pending code. If the problem is not found in a second drive cycle, the PCM judges that the system returned to normal or the problem was mistakenly detected, and deletes the pending code. If the problem is found in a second drive cycle too, the PCM judges that the system has failed, and the DTC is stored.