#
A-PILLAR TRIM REMOVAL/INSTALLATION

BHE091768160W01

1. Partially peel back the seaming welt.

2. Detach clips A using a fastener remover.

3. Pull the A-pillar trim and detach clip B (1).

4. Pull the A-pillar trim upward and remove clip B from the A-pillar trim (2).

5. Pull clip B out and rotate it 45°.

6. Remove clip B from the grommet by pulling it upward.

7. Install in the reverse order of removal.