#
DATA MONITORING AND RECORDING PROCEDURE

BHE092255430W06

1. Connect the WDS or equivalent to the diagnostic connector 2 (16-pin).

2. Verify the data monitor items.

## Indication Item Table

Monitor item | Input-output signal/part name | Unit/State | Terminal
--- | --- | --- | ---
CCNT_HE | DTC | Number of continuous DTCs | -
ECT_GAUGE | Water temperature gauge | °F | °C | 1J, 1L
FUEL | Fuel flow rate | l/min
ODO COUNT | Odometer | m
OPSC | Oil pressure gauge | -
SPEEDSG | Speedometer | mph | km/h
rpm | Tachometer | rpm