#
FUEL INJECTOR REMOVAL/INSTALLATION

BHE011413250W01

1. Follow the before repair procedure and perform fuel line safety procedure. (See BEFORE REPAIR PROCEDURE.)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

3. Remove the extension manifold (upper). (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

4. Remove the extension manifold (lower). (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

5. Remove the VDI actuator bracket installation bolt and the position the VDI actuator out of the way.

6. Disconnect the fuel injector connector.

7. Remove in the order indicated in the table.

1 | Quick release connector (See Inside the Engine Compartment.)
2 | Fuel distributor (housing side)
3 | Fuel distributor (intake manifold side)
4 | Fuel injector

8. Install in the reverse order of removal.

9. Inspect the variable dynamic effect intake (VDI) actuator. (See VARIABLE DYNAMIC EFFECT INTAKE-AIR (VDI) ACTUATOR INSPECTION.)

10. Inspect all parts by performing the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.)