#
DTC P0336

BHE010200300W06

DTC P0336 | Eccentric shaft position sensor circuit range/performance problem
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the eccentric shaft position sensor when the engine is running. If the input signal is not the proper pulse number, the PCM determines that there is a eccentric shaft position sensor circuit range/performance problem. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • PENDING CODE is available if the PCM detects the above malfunction condition. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Eccentric shaft position sensor malfunction • Connector or terminal malfunction • Eccentric shaft position sensor is dirty • Eccentric shaft position plate malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT ECCENTRIC SHAFT POSITION PLATE • Inspect the eccentric shaft position plate. (See ECCENTRIC SHAFT POSITION PLATE INSPECTION.) • Is there any malfunction? | Yes | Replace the eccentric shaft position plate, then go to Step 7. (See ECCENTRIC SHAFT POSITION PLATE REMOVAL/INSTALLATION.)
No | Go to the next step.
4 | INSPECT ECCENTRIC SHAFT POSITION SENSOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the eccentric shaft position sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 7.
No | Go to the next step.
5 | INSPECT ECCENTRIC SHAFT POSITION SENSOR • Inspect the eccentric shaft position sensor. (See ECCENTRIC SHAFT POSITION SENSOR INSPECTION.) • Is there any malfunction? | Yes | Replace the eccentric shaft position sensor, then go to Step 7. (See ECCENTRIC SHAFT POSITION SENSOR REMOVAL/INSTALLATION.)
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to the next step.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0336 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION.)
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE.) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE.)
No | DTC troubleshooting completed.