#
NEUTRAL SWITCH INSPECTION

BHE014017640W01

  Note

  • Before performing the following inspection, make sure to follow the troubleshooting flowchart. (See Troubleshooting Procedure.)

## Continuity Inspection

1. Remove the neutral switch.

2. Verify that the continuity between neutral switch terminals 1A and 2A is as indicated in the table.

  • If there is no malfunction, perform the "Circuit Open/Short Inspection".
  • If there is any malfunction, replace the neutral switch.

Measurement condition | Continuity
--- | ---
6MT | 5MT
Push the rod. | No continuity | Continuity detected
Except above | Continuity detected | No continuity

## Circuit Open/Short Inspection

1. Disconnect the PCM connector.

2. Disconnect the neutral switch connectors.

3. Inspect the following wiring harnesses for open or short circuit. (Continuity inspection)

### Open circuit

  • If there is no continuity in the following wiring harnesses, there is an open circuit. Repair or replace the wiring harness.
  – Neutral switch terminal 2A and PCM terminal 2O
  – Neutral switch terminal 1A and body ground

### Short circuit

  • If there is continuity in the following wiring harnesses, there is a short circuit. Repair or replace the wiring harness.
  – Neutral switch terminal 2A and body ground
  – Neutral switch terminal 2A and power supply