#
REAR FENDER PANEL REMOVAL

BHE098074100B01

  Caution

  • Avoid cutting with a blowtorch or similar tools as the insulator (shaded area) is flammable.

  Note

  • For weld location (A), partially bend back the rear end panel before drilling.

1. The rear fender panel and the rear pillar inner are joined with glue at the wheel arch line. Use a chisel or other to separate the rear fender panel from the rear pillar inner, then remove the rear fender panel.