#
FRAME REINFORCEMENT INSTALLATION

BHE098053342B02

1. When installing new parts, position each part so that the section measurement aligns with the body dimension.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

  Note

  • When replacing the frame reinforcement inner and the frame reinforcement outer separately, weld six weld locations indicated by (A).