#
DIFFERENTIAL OIL INSPECTION

BHE031427000W01

1. Position the vehicle on level ground.

2. Remove the oil-fill plug and the washer.

3. Inspect if the oil level is close to the rim of the oil-fill plug hole.

4. If the oil is not close to the rim of the oil-fill plug hole, add oil.

5. Install the oil-fill plug with a new washer and tighten.

  Tightening torque
  39.2-53.9 N·m {4.00-5.49 kgf·m, 29.0-39.7 ft·lbf}