#
AFTER REPAIR PROCEDURE

BHE011401006W04

  Warning

  • Fuel vapor is hazardous. It can very easily ignite, causing serious injury and damage. Fuel can also irritate skin and eyes. To prevent this, always complete the "Fuel Line Inspection".

## Fuel Leakage Inspection

  Warning

  • Fuel vapor is hazardous. It can very easily ignite, causing serious injury and damage. Fuel can also irritate skin and eyes. To prevent this, complete the following inspection with the engine stopped.

  Caution

  • Shorting the wrong terminal of the check connector may cause malfunctions. Make sure to short only the specified terminal.

1. Ground the check connector terminal F/P to the body using a jumper wire.

2. Turn the ignition switch to the ON position and operate the fuel pump.

3. Verify that there is no fuel leakage from the pressurized parts.

  • If there is leakage, replace the fuel hoses.
  • If there is damage to the seal on the fuel pipe side, replace the fuel pipe.

  Fuel Leakage
  There shall be no leakage after 5 min.

4. After reinstallation, repeat Step 1-3 of the fuel leakage inspection.