#
CLUTCH PEDAL REMOVAL/INSTALLATION

BHE051041030W02

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. Inspect and adjust the clutch pedal.

(See CLUTCH PEDAL ADJUSTMENT.)

1 | Clutch switch connector
2 | Clutch switch
3 | Nut cap
4 | Nut
5 | Retaining ring
6 | Joint pin
7 | Bush
8 | Nut
9 | Push rod
10 | Fork
11 | Pedal pad
12 | Clutch pedal component