#
SIMULATION TEST

BHE010200102T06

• The simulation items are shown below.

Simulation item table

×: Applicable
-: Not applicable

Item | Applicable component | Unit/condition | Test condition | PCM terminal
--- | --- | --- | --- | ---
KOEO | KOER
ACCS | A/C relay | On/Off | × | × | 5AA
AIP RLY | AIR pump relay | On/Off | × | × | 4O
ALTF | Generator (field coil) | % | - | × | 2I
APV | APV motor | On/Off | × | × | 3G, 3J
ARPMDES | Target engine speed | RPM | × | × | -
DEI | VDI solenoid valve | On/Off | × | × | 1W
ETC_DSD | Target throttle valve opening angle | ° | × | × | -
EVAPCP | Purge solenoid valve | % | × | × | 2P
FAN1 | Cooling fan relay No.1 | On/Off | × | × | 5X
FAN2 | Cooling fan relay No.2 | On/Off | × | × | 5AD
FP | Fuel pump relay | On/Off | × | × | 5P
FPRR | Fuel pump speed control relay | On/Off | × | × | 4M
FUELPW1 | Fuel injector (FP1, RP1) | % | - | × | 2J, 2M
GENVDSD | Target generator voltage | V | - | × | -
HTR12 | Rear HO2S heater | On/Off | × | × | 2A
IASV | VFAD solenoid valve | On/Off | × | × | 5Z
MOP_POS | Metering oil pump | - | × | × | 2V, 2W, 2Y, 2AB
PACNTV | AIR solenoid valve | On/Off | × | × | 1O
PREDELI | Delivery mode | On/Off | × | × | -
SSV | SSV solenoid valve | On/Off | × | × | 1L
test | Test mode | On/Off | × | × | -