#
FRONT TWEETER INSPECTION

BHE092066961W06

## Standard

1. Verify the resistance between front tweeter terminals.

  • If the continuity is as indicated in the table, replace the front tweeter.

2. Connect a 1.5 V battery to the front tweeter and verify that noise is sound from the front tweeter.

  • If no sound is output, replace the front tweeter.

## BOSE

1. Verify that sound is output from the front door speaker.

  • If sound is output, go to the next step.
  • If no sound is not output, inspect the front door speaker and the related wiring harnesses.

2. Remove the following parts:

  (1) Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Remove the tire house trim. (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Remove the rear pillar trim. (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (5) Remove the rear package center trim and the rear package side trim. (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)
  (6) Remove the main amplifier. (See AUDIO AMPLIFIER REMOVAL/INSTALLATION.)

3. Verify that the continuity between the front tweeter and the main amplifier is as indicated in the table.

  • If the continuity is not as indicated in the table, repair or replace the related wiring harnesses.
  • If the continuity is as indicated in the table, replace the front tweeter.