#
TRANSMISSION OIL INSPECTION [R15M-D]

BHE051127001W01

1. Position the vehicle on level ground.

2. Remove the filler plug.

3. Verify that the oil is near the brim of the plug port.

  • If the oil is not near the brim of the plug port, add the specified amount and type of oil.

  Specified oil
  API GL-4 or GL-5
  All season : SAE 75W-90
  Above 10°C {50 °F}: SAE 80W-90

4. Install a new filler plug.

  Tightening torque
  25-39 N·m {2.5-3.9 kgf·m, 18-28 ft·lbf}