#
CLOCK SPRING INSPECTION

BHE081066123W03

1. Remove the driver-side air bag module.

(See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

2. Remove the steering wheel.

(See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

3. Remove the clock spring. (See CLOCK SPRING REMOVAL/INSTALLATION.)

4. Verify continuity as indicated in the table.

  • If not as indicated in the table, replace the clock spring.

  Note

  • When the vehicle-side connector for the clock spring is disconnected, terminals 1A, 1B, 1C and 1D are shorted to prevent unexpected operation (deployment) of the air bag module.